**PLEASE NOTE… THIS DOCUMENT IS OUTDATED**

**Solution no longer requires Node-Red, document is here just for reference.**

**NEEO ZiggoNext (based on basst85/NextRemoteJs)**



1. Install the NextRemote package from Github containing the listener, according to below Github:

<https://github.com/basst85/NextRemoteJs>

2. Copy the modified index.js (included here) into the directory where NextRemoteJs is installed, replacing the existing one

3. Enter your Ziggo credentials in config.json

4. Run the listener-> pm2 start index.js

5. Copy ZiggoNext.json into

/steady/neeo-custom/.meta/node\_modules/@jac459/metadriver/Library

6. Goto node-red on your NEEO ip address: //ne.eo.ad.dr:1880 import Ziggoflow.json into node-red.

7. Install the Ziggodriver using meta